Implementation Guide
TI Terminology
Version 1.0.5-2 - release

## ValueSet: IHE XDS Language Code ValueSet für ePA

Official URL: https://gematik.de/fhir/terminology/ValueSet/epa-xds-language-code-vs | Version: 1.0.5-2
Active as of 2025-02-28 | Computable Name: EPAXDSLanguageCodeVS
Other Identifiers: OID:1.2.276.0.76.11.588 (use: official, )

Der Code, der die Sprache angibt, in der das Dokument verfasst ist.

References

This value set is not used here; it may be used elsewhere (e.g. specifications and/or implementations that use this content)

### Logical Definition (CLD)

Generated Narrative: ValueSet epa-xds-language-code-vs

- Include these codes as defined in `urn:ietf:bcp:47`

  Code | Display
  bg-BG | bulgarisch, Bulgarien
  it-IT | italienisch, Italien
  it-CH | italienisch, Schweiz
  cs-CZ | tschechisch, Tschechien
  lt-LT | litauisch, Litauen
  da-DK | dänisch, Dänemark
  lb-LU | luxemburgisch, Luxemburg
  de-AT | deutsch, Österreich
  de-DE | deutsch, Deutschland
  de-CH | deutsch,Schweiz
  de-LI | deutsch, Liechtenstein
  de-LU | deutsch, Luxemburg
  lv-LV | lettisch, Lettland
  el-GR | griechisch, Griechenland
  mt-MT | maltesisch, Malta
  en-AU | englisch, Australien
  en-GB | englisch, Vereinigtes Königreich
  en-CA | englisch, Kanada
  en-US | englisch, USA
  nl-NL | niederländisch, Niederlande
  nl-BE | niederländisch, Belgien
  es-ES | spanisch, Spanien
  no-NO | norwegisch, Norwegen
  et-EE | estnisch, Estland
  pl-PL | polnisch, Polen
  fi-FI | finnisch, Finnland
  pt-PT | portugiesisch, Portugal
  fr-CA | französisch, Kanada
  fr-FR | französisch, Frankreich
  fr-CH | französisch, Schweiz
  fr-LU | französisch, Luxemburg
  fr-BE | französisch, Belgien
  rm-CH | rätoromanisch, Schweiz
  ga-IE | irisch, Irland
  ro-RO | rumänisch, Rumänien
  hr-HR | kroatisch, Kroatien
  sk-SK | slowakisch, Slowakei
  hu-HU | ungarisch, Ungarn
  sl-SI | slowenisch, Slowenien
  is-IS | isländisch, Island
  sv-SE | schwedisch, Schweden

### Expansion

ValueSet

This value set contains 41 concepts

Code | System | Display (de-DE)
bg-BG | urn:ietf:bcp:47 |
it-IT | urn:ietf:bcp:47 |
it-CH | urn:ietf:bcp:47 |
cs-CZ | urn:ietf:bcp:47 |
lt-LT | urn:ietf:bcp:47 |
da-DK | urn:ietf:bcp:47 |
lb-LU | urn:ietf:bcp:47 |
de-AT | urn:ietf:bcp:47 |
de-DE | urn:ietf:bcp:47 |
de-CH | urn:ietf:bcp:47 |
de-LI | urn:ietf:bcp:47 |
de-LU | urn:ietf:bcp:47 |
lv-LV | urn:ietf:bcp:47 |
el-GR | urn:ietf:bcp:47 |
mt-MT | urn:ietf:bcp:47 |
en-AU | urn:ietf:bcp:47 |
en-GB | urn:ietf:bcp:47 |
en-CA | urn:ietf:bcp:47 |
en-US | urn:ietf:bcp:47 |
nl-NL | urn:ietf:bcp:47 |
nl-BE | urn:ietf:bcp:47 |
es-ES | urn:ietf:bcp:47 |
no-NO | urn:ietf:bcp:47 |
et-EE | urn:ietf:bcp:47 |
pl-PL | urn:ietf:bcp:47 |
fi-FI | urn:ietf:bcp:47 |
pt-PT | urn:ietf:bcp:47 |
fr-CA | urn:ietf:bcp:47 |
fr-FR | urn:ietf:bcp:47 |
fr-CH | urn:ietf:bcp:47 |
fr-LU | urn:ietf:bcp:47 |
fr-BE | urn:ietf:bcp:47 |
rm-CH | urn:ietf:bcp:47 |
ga-IE | urn:ietf:bcp:47 |
ro-RO | urn:ietf:bcp:47 |
hr-HR | urn:ietf:bcp:47 |
sk-SK | urn:ietf:bcp:47 |
hu-HU | urn:ietf:bcp:47 |
sl-SI | urn:ietf:bcp:47 |
is-IS | urn:ietf:bcp:47 |
sv-SE | urn:ietf:bcp:47 |

Explanation of the columns that may appear on this page:

Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies
System | The source of the definition of the code (when the value set draws in codes defined elsewhere)
Code | The code (used as the code in the resource instance)
Display | The display (used in the display element of a Coding). If there is no display, implementers should not simply display the code, but map the concept into their application
Definition | An explanation of the meaning of the concept
Comments | Additional notes about how to use the code